



Low pass filter with cut-off frequency 4 kHz